#-
# Copyright (c) 2014 Luiz Otavio O Souza <loos@FreeBSD.org>
# All rights reserved.
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in the
#    documentation and/or other materials provided with the distribution.
#
# THIS SOFTWARE IS PROVIDED BY THE REGENTS AND CONTRIBUTORS ``AS IS'' AND
# ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
# IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
# ARE DISCLAIMED.  IN NO EVENT SHALL THE REGENTS OR CONTRIBUTORS BE LIABLE
# FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
# DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS
# OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
# HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY
# OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF
# SUCH DAMAGE.
#
# $FreeBSD: stable/12/usr.sbin/bsnmpd/modules/snmp_lm75/lm75_tree.def 266936 2014-06-01 03:14:03Z loos $
#

(1 internet
  (4 private
    (1 enterprises
      (12325 fokus
        (1 begemot
          (400 begemotLm75
            (1 begemotLm75Objects
              (1 lm75Sensors
                (1 lm75Sensors INTEGER32 op_lm75Sensors GET)
              )
              (2 lm75SensorTable
                (1 lm75SensorEntry : OCTETSTRING op_lm75SensorTable
                  (1 lm75SensorIndex INTEGER32 GET)
                  (2 lm75SensorSysctlIndex INTEGER32 GET)
                  (3 lm75SensorDesc OCTETSTRING GET)
                  (4 lm75SensorLocation OCTETSTRING GET)
                  (5 lm75SensorPnpInfo OCTETSTRING GET)
                  (6 lm75SensorParent OCTETSTRING GET)
                  (7 lm75SensorTemperature INTEGER32 GET)
                )
              )
            )
          )
        )
      )
    )
  )
)
